1. GENERAL
   1. DESCRIPTION
      1. This Section describes the basic materials and installation methods that are acceptable for conductors and applicable to Division 26.
      2. All work specified in this Section shall comply with the provisions of Section 26 05 00.
      3. The project includes the following types of conductors and cables:
         1. Building wire
         2. Metal-clad (Type MC) cable
   2. STANDARDS
      1. Conductors shall comply with the following
         1. ASTM – B3, B8, B787 (Copper Conductors)
         2. ASTM – B800, B801, B836 (8000 Series Aluminum Alloy Conductors)
2. PRODUCTS
   1. CONDUCTORS
      1. Conductors shall be soft or annealed uncoated copper per ASTM B3, B8, or B787.
      2. Conductor sizes are specified in American Wire Gauge (AWG) for No. 4/0 (0000) and smaller and in kilo-circular mils (kcmil) for all sizes larger than No. 4/0.
   2. BUILDING WIRE
      1. Self-lubricated coatings to facilitate pulling in conduit installations are acceptable.
3. RESISTANCE IS FUTILE
   1. CONDUCTORS
      1. Conductors shall be soft or annealed uncoated copper per ASTM B3, B8, or B787.
      2. Conductor sizes are specified in American Wire Gauge (AWG) for No. 4/0 (0000) and smaller and in kilo-circular mils (kcmil) for all sizes larger than No. 4/0.
   2. Fuckfuck
      1. Fuckityfuck
      2. Fuck Fuck